{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Parts List"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":5,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Parts List","index":0,"n_rows":120,"n_cols":14,"rows_kept":120,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Updated","Qty","Value","Reference","Description / Comments","Vendor","Vendor P/N","Mfgr","Cost ea.","Cost"]
[null,"RECEIVER"]
["Yes - Mouser",7,0.1,"C1,C4,C15,C18,C27,C32,C33","Ceramic, Z5U","Mouser","21RZ310","Xicon",0.08,0.56]
["Yes - Digikey",6,0.01,"C2,C8,C9,C10,C13,C16",null,"Digi-Key","P4582-ND","Panasonic","10 / $.78",0.78]
["NO",3,"220pf","C3,C6,C11",null,"Mouser","140-CD50S5-221J","Xicon",0.08,0.24]
["NO",1,"390pf","C5",null,"Mouser","140-CD50S5-391J","Xicon",0.09,0.09]
["Yes - Mouser",1,0.0022,"C12",null,"Mouser","140-PF2A222J","Xicon",0.12,0.12]
["NO",1,"47pf","C14",null,"Mouser","140-CD50S2-047J","Xicon",0.07,0.07]
["Yes - Mouser",1,0.0047,"C17",null,"Mouser","140-PF2A472J","Xicon",0.12,0.12]
["NO",2,"1.0","C19,C35","Tantalum","Digi-Key","P2105","Panasonic",0.28,0.56]
["Yes - Mouser",1,".047","C20",null,"Mouser","140-PF2A473J","Xicon",0.21,0.21]
["Yes - Mouser",2,".0047","C21,C22",0.02,"Mouser","140-PF2A472F","Xicon",0.51,1.02]
["Yes - Mouser",2,".01","C23,C24",0.02,"Mouser","140-PF2A103F","Xicon",0.51,1.02]
["Yes - Mouser",2,".0068","C25,C26",0.02,"Mouser","140-PF2A682F","Xicon",0.51,1.02]
[null,2,"18pf","C28,C29","NPO","Mouser","141-100N2-018J","Xicon",0.09,0.18]
["NO",1,"10uf","C30","Tantalum, 6.3V","Digi-Key","P2013","Panasonic",0.39,0.39]
["Yes - Mouser",2,"220uf","C31,C34","Elect, 10V","Mouser","140-XRL10V220-RC","Xicon",0.08,0.16]
[]
["Yes - eBay",1,"MVAM109","D1","Tuning Diode","eBay",null,"Motorola",3,3]
["Yes - Digikey",1,"MA198CT","D2A,D2B","Dual diode (SM)","Digi-Key","MA3J14300LCT-ND","Panasonic",0.41,0.41,null,null,null,"?"]
["Stock",4,"1N4148","D3,D4,D5,D6",null,"Mouser","583-1N4148",null,0.04,0.16]
["Stock",1,"HLMP-1700","D7","LED","Digi-Key","HLMP-1700QT","QT Opto",0.3,0.3]
[]
[null,2,"DF13-3S","P1,P2  (mate to J1, J2)","3-pin connector  (Note 1)","Digi-Key","H2180","Hirose",0.13,0]
[null,3,"DF13-2S","P3,P4,P5  (mate to J3 - J5)","2-pin connector","Digi-Key","H2179","Hirose",0.13,0]
[null,2,"DF13-3P","J1,J2","3 pin header","Digi-Key","H2192","Hirose",0.27,0]
[null,3,"DF13-2P","J3,J4,J5","2 pin header","Digi-Key","H2191","Hirose",0.22,0]
[null,null,null,"n/a","Contacts for P1-P4","Digi-Key","H9992","Hirose","100/$3.45",0]
[{"$nulls":9},0]
["Yes - Mouser",1,"6.8mH","L1","Could substitute 4.7mH","Mouser","43LH268","Xicon",1.05,1.05]
["Yes - Mouser",3,"1.0mH","L2,L3,L4","Alternate P/N: 434-06-102J","Mouser","43LS103","HiQ",0.41,1.23]
[{"$nulls":9},0]
["Yes - Mouser",1,"2N4393","Q1","Could use MPF4393 also","Mouser","610-2N4393",null,1.89,1.89]
["Yes - Mouser",4,"2N5210","Q2,Q3,Q5,Q6",null,"Mouser","610-2N5210",null,0.28,1.12]
["Yes - Mouser",1,"2N5484","Q4",null,"Mouser","610-2N5484",null,0.68,0.68]
[]
["Yes - Digikey",3,"100k","R1,R34,R35",null,"Digi-Key","100KQBK",null,"5 / $.58",0.58]
["Digikey",4,"220k","R2,R13,R14,R15",null,"Digi-Key","220KQBK",null,"5 / $.28",0.28]
["Digikey",2,"562k","R3,R21","1%   R3 can be 560k, 5%","Digi-Key","562KXBK",null,"5 / $.54",0.54]
["Digikey",1,"4.7k","R4",null,"Digi-Key","4.7KQBK",null,"5 / $.28",0.28]
["Digikey",2,"20k","R5,R6",null,"Digi-Key","20KQBK",null,"5 / $.28",0.28]
["Digikey",5,"33k","R9,R17,R18,R28,R40",null,"Digi-Key","33KQBK",null,"5 / $.28",0.28]
["Digikey",1,"13k","R10",null,"Digi-Key","13KQBK",null,"5 / $.28",0.28]
["Digikey",2,"6.8k","R11,R29",null,"Digi-Key","6.8KQBK",null,"5 / $.28",0.28]
["Digikey",2,"150","R12,R36",null,"Digi-Key","150QBK",null,"5 / $.28",0.28]
["Digikey",3,"51k","R16,R32,R39",null,"Digi-Key","51KQBK",null,"5 / $.28",0.28]
["Digikey",1,"56.2k","R19",0.01,"Digi-Key","56.2KXBK",null,"5 / $.54",0.54]
["Digikey",1,"10.0k","R20",0.01,"Digi-Key","10.0KXBK",null,"5 / $.54",0.54]
["Digikey",2,"39.2k","R22,R25",0.01,"Digi-Key","39.2KXBK",null,"5 / $.54",0.54]
["Digikey",3,"2.49k","R23,R26,R33","1%    R33 can be 2.2k, 5%","Digi-Key","2.49KXBK",null,"5 / $.54",0.54]
["Digikey",2,"665k","R24,R27",0.01,"Digi-Key","665KXBK",null,"5 / $.54",0.54]
["Digikey",1,"68k","R30",null,"Digi-Key","68KQBK",null,"5 / $.28",0.28]
["Digikey",1,"270k","R31",null,"Digi-Key","270KQBK",null,"5 / $.28",0.28]
["Digikey",2,"1k","R37,R38",null,"Digi-Key","1KQBK",null,"5 / $.28",0.28]
["Digikey",1,"3.3M","R41",null,"Digi-Key","3.3MQBK",null,"5 / $.28",0.28]
[]
["Yes - Mouser",2,"42IF203","T1,T3","7mm, 455kHz IF Transformer","Mouser","42IF203",null,1.16,2.32]
["Yes - Mouser",2,"42IF201","T2,T4","7mm, 455kHz IF Transformer","Mouser","42IF201",null,1.16,2.32]
[]
["Yes - Digikey",1,"LMC660","U1","Quad Op Amp","Digi-Key","LMC660CN-ND","National",2.14,2.14]
["Yes - Mouser",1,"TLC3702","U2","Dual Comparator","Digi-Key","296-1841-5-ND","TI / SGS",0.94,0.94]
["Yes - Mouser",1,"NE602A","U3","Mixer/Oscillator","Digi-Key","568-1201-5-ND","Philips",2.43,2.43]
["NO",1,"MC145157","U4","PLL Synthesizer","Future/Active","MC145157P2","Motorola",7.22,7.22]
[null,1,"PIC16C76","U5","Microcontroller   (Note 2)","Digi-Key","PIC16C76/JW","Microchip",15.86,15.86]
["Yes - Digikey",1,"93LC46B","U6","EEPROM","Digi-Key","93LC46B/P-ND","Microchip",0.46,0.46]
["Yes - Digikey",1,"28 pin x 0.3\"","Socket for U5",null,"Digi-Key","3M5480-ND",null,0.32,0.32]
["Yes - Digikey",1,"4.00 MHz","Y1",null,"Digi-Key","SER3404-ND","Epson CA-301",2.69,2.69]
[null,1,"PCB",null,"PCB","Note 3",null,null,null,0]
[{"$nulls":8},"TOTAL",60.26000000000001]
[null,"LOOPSTICK ANTENNA"]
[null,1,null,"L1","Ferrite Rod","ByteMark","R33-037-400","Amidon",4,4]
[null,"20'",null,null,"8/44 Litz Wire (optional)","ByteMark","#8/44 LITZ WIRE",null,"0.05/ft",1]
[null,1,"220pf","C3",null,"Mouser","140-CD50S2-221J","Xicon",0.08,0.08]
[null,1,0.0022,"C2",null,"Mouser","140-PF2A222J","Xicon",0.12,0.12]
[null,3,0.1,"C1,C4,C5","Ceramic, Z5U","Mouser","21RZ310","Xicon",0.08,0.24]
[null,1,"MVAM109","D1","Tuning Diode","Tech-Am",null,"Motorola",0.85,0.85]
[null,1,"2N4393","Q1","Could use MPF4393 also","Mouser","610-2N4393",null,1.11,1.11]
[null,1,"2N5210","Q2",null,"Mouser","610-2N5210",null,0.28,0.28]
[null,1,"100k","R1",{"$nulls":5},0]
[null,1,"270k","R2",{"$nulls":5},0]
[null,1,"6.8k","R3",{"$nulls":5},0]
[null,1,"220k","R4",{"$nulls":5},0]
[{"$nulls":8},"TOTAL",7.680000000000001]
[null,"WHIP ANTENNA"]
["Yes - Mouser",3,0.1,"C1,C2,C4","Ceramic, Z5U","Mouser","21RZ310","Xicon",0.08,0.24]
[null,1,"220pf","C3",null,"Mouser","140-PF2A222J","Xicon",0.12,0.12]
["no",1,"1.0uf","C5","Tantalum","Digi-Key","P2105","Panasonic",0.28,0.28]
["Yes - Mouser",1,"42IF201","L1","455kHz IF Transformer","Mouser","42IF201",null,1.16,1.16]
[null,1,"6.8mH","L2","Could substitute 4.7mH","Mouser","434-06-682J","Xicon",1.07,1.07]
[null,1,"NE-38S","LP1","Could use NE-2","Mouser","602-2ML","Chicago",0.9,0.9]
[null,1,"2N5484","Q1",null,"Mouser","610-2N5484",null,0.55,0.55]
[null,1,"2N5210","Q2",null,"Mouser","610-2N5210",null,0.28,0.28]
[null,1,"100k","R1",null,"Digi-Key","100KQBK",null,null,0]
[null,1,"270k","R2",null,"Digi-Key","270KQBK",null,null,0]
[null,1,"1M","R3","Can use 665k 1%","Digi-Key",null,null,null,0]
[null,1,"4.7k","R4",null,"Digi-Key","4.7KQBK",null,null,0]
[null,1,"10k","R5",null,"Digi-Key","10KQBK",null,null,0]
[null,1,"33k","R6",null,"Digi-Key","33KQBK",null,null,0]
[{"$nulls":8},"TOTAL",4.6000000000000005]
[null,"POWER SUPPLY"]
[null,1,"0.1","C1","Ceramic, Z5U","Mouser","21RZ310","Xicon",0.08,0.08]
[null,1,"1uf","C2","Tantalum","Digi-Key","P2105","Panasonic",0.28,0.28]
[null,1,"LP2950ACZ-5.0","U1","LDO Regulator","Digi-Key","LP2950ACZ-5.0","National",1.58,1.58]
[]
[{"$nulls":9},1.9400000000000002]
[null,"GENERAL NOTE:  See the Construction Document for additional information on some of the parts, including substitution and options."]
[]
[null,"NOTES:"]
[null,1,"The DF13 PCB connectors can be used in place of soldering wires directly to the PCB, adding about $5 to the cost. See Construction Document for more information."]
[null,2,"See Construction Document for microcontroller options. The one listed is the most versatile, but most expensive."]
[null,3,"For list of current PCB sources, see http://home1.gte.net/clseng/dgps/pcb_info.txt"]
[]
[null,"Vendor Links:",null,"http://www.future-active.com/","Might also carry MVAM109, MPF4393"]
[null,null,null,"http://www.digi-key.com/","Also carries LMC660"]
[null,null,null,"http://www.mouser.com/"]
[null,null,null,"http://www.cl.ais.net/farcir/","One source for PCB"]
[null,null,null,"http://www.techam.com/","Alternate source for SA602A"]
[]
[null,"Other Vendors:",null,"http://www.jdr.com/","Alternate source for SA602A"]
[null,null,null,"http://www.newark.com/","Also carries TLC3702, MC145157, SA602"]